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	Column Splice Flange Connection Checklist



	Project: COV-TEN-CON 514 – Stack Raise Installation, Kwinana Lithium Refinery
	Client: Covalent Lithium

	Description: 
	Area Ref:

	Marking Plan/s Ref: 
	ITP No: 

	Module Reference:
	WP No: 

	Item
	Item Description
	Installer
	Verified

	SRG Super 

	1
	Correct module, column/leg and column splice flange interface identified against drawings and marking plan.
	
	
	

	2
	Column splice flange faces clean, undamaged and free from coating build-up or debris.
	
	
	

	3
	Correct shim pack installed at each leg/interface in accordance with survey/alignment requirements.
	
	
	

	4
	Shim thickness recorded, any deviation from nominal shim pack captured and approved where required.
	
	
	

	5
	Temporary alignment pins/drift pins tethered control during landing and alignment.
	
	
	

	6
	Temporary alignment pins removed progressively and replaced with permanent bolts.
	
	
	

	7
	Correct bolts, nuts and washers installed, size, grade and coating verified against MTO/specification.
	
	
	

	8
	Bolt holes aligned, no forced fit, or modification undertaken.
	
	
	

	9
	Local level completed at column splice flange interface prior to final tensioning.
	
	
	

	10
	Survey/verticality record referenced and accepted prior to final bolt tensioning.
	
	
	

	11
	Final bolt tension completed to specified Orientation using calibrated tooling.
	
	
	

	12
	Connection visually inspected, no unacceptable gaps, distortion or damage evident.
	
	
	

	Shims Thickness Recorded
	
	
	
	

	
				Top/North
		
		Section 4			Section 1
	
		    West			                    East



		Section 3			Section 2


			       
                                                
                                                 Bottom/South

 

	Comments/Punch List Items




	Attachments



	Verified by: 

					/       /
	Reviewed by Client: 

						/      /
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