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	Stack Flange Connection Checklist



	Project: COV-TEN-CON 514 – Stack Raise Installation, Kwinana Lithium Refinery
	Client: Covalent Lithium

	Description: 
	Area Ref:

	Marking Plan/s Ref: 
	ITP No: 

	Module Segment Reference:
	WP No: 

	Item
	Item Description
	Installer
	Verified

	SRG Super 

	1
	Correct stack segment / flange ID installed as per drawings and marking plan.
	
	
	

	2
	Flange faces clean, undamaged and free from coating build-up or debris.
	
	
	

	3
	Correct gasket installed type, thickness and orientation verified.
	
	
	

	4
	Correct bolts, nuts and washers installed, size, grade and coating verified against MTO/specification.
	
	
	

	5
	Bolt holes aligned, no forced fit, unauthorised reaming or modification undertaken.
	
	
	

	6
	Temporary supports, lifting guides and closure beams installed/removed as required 
	
	
	

	7
	Initial snug tightening completed prior to final torque/tensioning.
	
	
	

	8
	Final bolt tensioning completed to specified nut orientation using calibrated tooling
	
	
	

	9
	Flange gap, squareness/alignment and visual fit-up acceptable prior to release.
	
	
	

	10
	Restraints installed as required.
	
	
	

	11
	Survey completed and accepted for the installed stack segment.
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	Comments/Punch List Items




	Attachments



	Verified by:                                             /       /
	Reviewed by Client:                               	/      /
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