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	Structural Splice / Gusset / Fish Plate Connection Checklist



	Project: COV-TEN-CON 514 – Stack Raise Installation, Kwinana Lithium Refinery
	Client: Covalent 

	Description: 
	AREA Ref:

	Marking Plan/s Ref: 
	ITP No: 

	Module Reference:
	WP No: 

	Item
	Item Description
	Installer
	Verified

	SRG Super 

	1
	Correct structural member / brace installed at nominated location as per drawings and marking plan.
	
	
	

	2
	Correct fish plates, gusset plates, cleats and connection plates installed and orientated correctly.
	
	
	

	3
	Connection faces clean and free from debris, or coating build-up affecting fit-up.
	
	
	

	4
	Bolt holes aligned, no flame cutting or modification undertaken.
	
	
	

	5
	Correct bolts, nuts and washers installed, size, grade and coating verified against MTO/specification.
	
	
	

	6
	Temporary bolts/alignment pins removed where not part of permanent connection.
	
	
	

	7
	Connection snug tightened during assembly / fit-up prior to final tensioning.
	
	
	

	8
	Final bolt tensioning completed to specified rotation using calibrated tooling
	
	
	

	9
	Connection visually inspected, member seated correctly with no gaps or distortion.
	
	
	

	10
	Punch list or repair/deviation approval raised where defects or unauthorised modifications are identified.
	
	
	

	

#1☐

#3 ☐
#2 ☐














	Comments/Punch List Items




	Attachments



	Verified by: 

					/       /
	Reviewed by Client: 

						/      /
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